# Using Update

To do an update of a Cube two scripts are available allowing to perform a remote (from the Array Cointroller) and a local update (on the Cube).

## Remote Update

If you are making a remote update, follow these procedures:

1. Copy the following files to the Array Controller to the directory /update:

update.sh, update-remote.sh and update.tar

1. Execute in /update: **chmod 777 \*.sh**
2. Run in /update update.sh as:

update.sh <IP address> <root password> <Cube type>

The Cube type can be:

AC = Air Cooled

LC-LD = Liquid Cooled - Long Duration

LC-SD = Liquid Cooled - Short Duration

For instance:

**update.sh 10.11.9.101 admin LC-LD**

## Local Update

If you are making a local update, follow these procedures:

1. Copy the following files to the Cube to the directory /update:

update-remote.sh and update.tar

1. Execute in /update: **chmod 777 \*.sh**
2. Run in /update update-remote.sh as:

update-remote.sh <Cube type>

The Cube type can be:

AC = Air Cooled

LC-LD = Liquid Cooled - Long Duration

LC-SD = Liquid Cooled - Short Duration

For instance:

**update-remote.sh AC**