# Using Update

To do an update of a Cube 2 scripts are available allowing to perform a remote and a local update

## Remote Update

If you are making a remote update transfer the following files to the Array Controller.

update.sh, update-remote.sh and update.tar.

Run update.sh as:

update.sh <IP address> <root password> <cube type>

The Cube type can be:

AC = Air Cooled LC-LD = Liquid Cooled - Long Duration LC-SD = Liquid Cooled - Short Duration

For instance:

update.sh 10.11.9.101 admin LC-LD

## Local Update

If you are making a local update transfer these files to the Cube.

update-remote.sh and update.tar.

Run update-remote.sh as:

update-remote.sh <cube type>

The Cube type can be:

AC = Air Cooled LC-LD = Liquid Cooled - Long Duration LC-SD = Liquid Cooled - Short Duration

For instance:

update-remote.sh AC